ALU

A

B

B

A

Addr

Addr

Val

= Control Register

= Data gate

= 8 Bit Width

Extends Down if Needed

RAM

(Single Read)

16b

Data I/O

Extends Down if Needed

ROM

Registers (Dual Read) + Program Counter

Control Unit + Clock